LOCKERS
(30018, 30024)

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	24-inch Wide Open Access Designer Wood Lockers.

1.2	REFERENCES
A.	IBC - International Building Code.
B.	LEED Submittal Requirements NC v3.0:  Sustainable Design Requirements – LEED for New Construction and the LEED NC v3.0 reference guide.

1.3	RELATED SECTIONS
A.	Section 06114 - Wood Blocking and Curbing; Wood grounds and attachment strips.
B.	Section 06200 - Finish Carpentry:  Related trim not specified in this section.

1.4	SUBMITTALS
A.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
B.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
C.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
D.	Submit under provisions of LEED NC v3.0 reference guide:  Product data for each type of accessory specified, with installation instructions for each unit built-in or connected to other construction:
1.	Product Data for Credit MR 4 – Recycled Content:  For products having recycled content, documentation indicating percentages by weight of post-consumer and pre-consumer recycled content.
2.	Product Data for Credit MR 5 – Regional Materials:  Provide documentation indicating where materials have been extracted, harvested or recovered, as well as manufactured.  If only a portion of the product has been extracted, harvested or recovered, and manufactured within 500 miles of the job site, then indicate that percentage.
3.	Product Data for IEQ 4.1 – Low Emitting Materials-Adhesives and Sealants:  Provide documentation including printed statement of VOC content for all adhesives and sealants.
4.	Product Data for Credit IEQ 4.2:   Submit product data and MSDS for interior paints and coatings, verifying VOC levels and compliance for Green Seal Standard GS-11, GC-03 and SCAQMD Rule 1113.
5.	Laboratory Test Reports for Credit IEQ 4.2:  For primers, documentation indicating that products comply with the testing and product requirements of the California Department of Health Services’ “Standard Practice for the Testing of Volatile Organic Emissions from Various Sources Using Small-Scale Environmental Chambers”.

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging, in a dry, ventilated area until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS

2.1	LOCKERS
24-inch wide open access designer wood lockers:  Constructed of industrial grade particleboard and covered with durable plastic laminate; includes a lift up handle and recessed hasp for added security; can accommodate built-in combination or key locks, combination or key padlocks, resettable combination locks or electronic locks.  Lockers are available as fully assembled units only and require minor assembly.

A.	24-inch Wide Open Access Designer Wood Locker Models:
1.	30018.
2.	30024.

B.	Unit Width:  24 inches (610 mm).

C.	Unit Height:
1.	76 inches (1,930 mm) with bases.
2.	72 inches (1,828 mm) without bases.

D.	Unit Depth:
1.	18 inches (457 mm).
		3.	24 inches (610 mm).

E.	Unit Assembly:  Requires minor assembly.

F.	Laminate Color: 
1.	Color: Gray - standard.
2.	Color: Blue - standard.
	3.	Color: Black - standard.
	4.	Color: Maple - standard.
	5.	Color: Cherry - standard.
	6.	Color: Mahogany - standard.

2.2	INTERIOR EQUIPMENT

A.	Standard Hardware Features: 
		1.	One steel recessed padlock hasp on top storage compartment door.
		2.	One 11 inch wide x 12 inch high x 15-1/2 inch deep
(279 mm wide x 305 mm high x 394 mm deep)
			top storage compartment in 18 inch deep lockers;
.			one 11 inch wide x 12 inch high x 21-1/2 inch deep
(279 mm wide x 305 mm high x 546 mm deep)
			top storage compartment in 24 inch deep lockers
		3.	Two wall-mounted, single-prong stainless steel coat hooks.
		4.	One stainless steel coat rod.
		5.	One 16-3/4 inch (425 mm) deep upper shelf in 18 inch deep lockers;
one 22-3/4 inch (578 mm) deep upper shelf in 24 inch deep lockers.
		6.	One 14 inch (356 mm) high foot locker with a hinged lid, vented front panel			and padlock hasp.

2.3	OPTIONAL EQUIPMENT

	A.	Sloping hoods:
		1.	24 inches (610 mm) for 1-wide units.

B.	Bases:  4 inches (102 mm) high.

C.	Side panels:
	1.	Without sloping hoods.
	2.	With sloping hoods.

D.	Built-In Locks:
	1.	Built-in combination locks.
	2.	Built-in keyed locks.
	3.	Built-in resettable combination locks.
	4.	Built-in electronic locks.

E.	Padlocks:
	1.	Combination padlocks.
	2.	Keyed padlocks.

F.	Master keys:
	1.	Master control key for built-in combination locks.
	2.	Master control key for built-in keyed locks.
	3.	Master control key for built-in resettable combination locks.
	4.	Master control key for combination padlocks.

G.	Engraved name/number plates.

2.4	CUSTOMIZATION

A.	Custom colors – For all custom colors available, contact Salsbury Industries or visit www.lockers.com/customdesignerlockers:
	1.	Minimum order of ten locker frames.

2.5	CONSTRUCTION
A.	Locker Body – Tops, bottoms, sides, backs and shelves are precision machined:
1.	Locker shall be fabricated using doweled and glued assembly process.
2. 	Tops and bottoms with three sides formed to 90 degrees, the front offset formed to be flush with horizontal frame member.
3.	Shelves with four sides formed to 90 degrees.

B.	Locker Top Compartment Door – Door is precision machined: 
1.	Door:
		a.	Door has four radial edges.
		b.	Routed inset to insert and attach number plates.
2.	Ventilation – 1/2 inch (12.7 mm) opening between door and frame on locker top and bottom provide unrestricted airflow.
3.	Single-point latching:
			a.	Recessed handle in door.
			b.	Integral Pocket and Pull:  22 gauge powder coated stainless 					steel securely fastened to door with two lugs and a positive 					tamper-resistant decorative fastener.
I.	Pocket Depth:  Sufficient to prevent a combination padlock,
built-in combination lock, or key lock from protruding beyond door face.
				II.	Pull:  Formed in pocket.
				III.	Padlock Staple:  Protruding through pocket.
			c.	Provide lock hole cover plate for use with padlocks.
			d.	Locking Device:  11 gauge steel hasp welded to locker frame; 					include surface for engaging the bolt of a built-in combination 					or key lock and anti-pry lug and slot to deter prying open when locked.
			e.	Firmly secure rubber silencers to locker frame.
C.	Fabricate locker parts square, rigid and without warp, with the finished faces flat and free of scratches and chips.
D.	Fabricate corners and fillers as required for installation.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industry's installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.
C.	Lockers can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION