LOCKERS
(70018, 70024)

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	24-inch Wide Open Access Standard Metal Lockers.

1.2	REFERENCES

A.	IBC - International Building Code.

1.3	RELATED SECTIONS
	
A.	Section 03300 (03 30 00) – Cast-in-Place Concrete:  Concrete bases.
B.	Section 06100 (06 10 00) – Rough Carpentry:  Wood ground and furring for anchoring lockers.
C.	Section 09650 (09 65 13.13) – Resilient Base.

1.4	SUBMITTALS
A.	Submit under provisions of Section 013300.
B.	Product Data - Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
D.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns. 

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion. 

PART 2    PRODUCTS

2.1	LOCKERS
24-inch wide open access standard metal lockers:  Constructed of 16 gauge steel; durable powder coated finish; top compartment includes a lift up handle and recessed hasp for added security; top compartment can accommodate built-in combination locks, built-in key locks, combination padlocks or key padlocks, and foot locker compartment can accommodate combination padlocks or key padlocks.

A.	24-inch Wide Open Access Standard Metal Locker Models:
		1.	70018.
		2.	70024.

B.	Unit Width:  24 inches (610 mm).

C.	Unit Height:  72 inches (1,828 mm).

D.	Unit Depth: 
		1.	70018:  18 inches (457 mm).
		2.	70024:  24 inches (607 mm).

E.	Unit Assembly: 
		1.	Unassembled units (Knocked-down).
		2.	Assembled units.

F.	Unit Color: 
		1.	Color: Gray - standard.
		2.	Color: Tan - standard.
		3.	Color: Blue - standard.

2.2	INTERIOR EQUIPMENT
	
A.	Standard Hardware Features: 
		1.	One steel recessed padlock hasp on top storage compartment door.
		2.	One 12 inch wide x 12-1/2 inch high x 13-3/4 inch deep
(305 mm wide x 318 mm high x 349 mm deep)
			top storage compartment.
		3.	Two wall-mounted, single-prong stainless steel coat hooks.
		4.	One stainless steel coat rod.
		5.	One 13-3/4 inch (349 mm) deep upper shelf.
		6.	One 14 inch (356 mm) high foot locker with a hinged lid, vented front panel			and padlock hasp.

2.3	OPTIONAL EQUIPMENT

A.	Built-In Locks (for top storage compartment): 
		1.	Built-in combination locks.
	2.	Built-in keyed locks.

B.	Padlocks (for top storage compartment and foot locker):
	1.	Combination padlocks.
	2.	Keyed padlocks.

C.	Master keys: 
	1.	Master control key for built-in combination locks.
	2.	Master control key for built-in keyed locks.
	3.	Master control key for combination padlocks.

D.	Engraved name/number plates.

2.4	CONSTRUCTION
A.	Locker Doors:  Steel specially formed for added strength and rigidity and to ensure tight joints at fastening points.
	1.	Door:  16 gauge - .060 inch (1.52 mm) thick steel.
2.	Ventilation:
a. 	Top storage compartment:  Solid facing.
b.	Foot locker  compartment:  Ventilated facing.
3.	Single-point latching:
a.	Top storage compartment door:  Recessed handle; integral pocket and pull made of stainless steel securely fastened to door and sufficient to prevent a combination padlock, built-in combination lock, or key lock from protruding beyond door face.
b.	Foot locker door:  One-point locking device with a steel lock clip for 		attaching padlock.
B.	Locker Body:  Solid steel specially formed for added strength and rigidity and to ensure tight joints at fastening points.
C.	Hinges:
1.	Top storage compartment door hinges: 0.074 inch (1.88 mm) thick sheet steel, double spun, full loop, tight pin, projection welded to door frame and securely fastened to compartment door; two 2 inch (51 mm) high five-knuckle hinges installed on compartment door.
2.	Foot locker door hinge:  16 gauge continuous hinge secured with rivets to door frame and to door. Hinge has 1/2 inch (12.7 mm) knuckles and 0.235 inch (5.969 mm) diameter.
D.	Optional factory assembly of locker bodies using heavy duty steel rivets.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industries’ installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.
C.	Lockers can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION