LOCKER BENCHES
(77770, 77771)

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Aluminum Locker Benches.
B.	Aluminum ADA Locker Benches.

1.2	REFERENCES
A.	ADAAG - Americans with Disabilities Act, Accessibility Guidelines.
B.	IBC - International Building Code.

1.3	RELATED SECTIONS

A.	Section 03300 (03 30 00) – Cast-in-Place Concrete:  Concrete bases.
B.	Section 06100 (06 10 00) – Rough Carpentry:  Wood ground and furring for anchoring lockers.
C.	Section 09650 (09 65 13.13) – Resilient Base.

1.4	SUBMITTALS
A.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
B.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging, in a dry, ventilated area until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS

2.1	LOCKERS
Standard and ADA-compliant aluminum locker benches:  Constructed entirely of aluminum that is 1-3/4” (44 mm) thick; includes two 3 inch (76 mm) diameter bolt mounted pedestals in an aluminum powder coated finish; pedestals include four (4) mounting holes to secure to the ground; combines a classic look with strength and durability. Requires minor assembly.

A.	Aluminum Locker Bench Series:
1.	77773:  36” Wide (914 mm) Wood Locker Bench.
2.	77774:  48” Wide (1,219 mm) Aluminum Locker Bench.
3.	77775:  60” Wide (1,524 mm) Aluminum Locker Bench.
4.	77776:  72” Wide (1,829 mm) Aluminum Locker Bench.
5.	77777:  84” Wide (2,134 mm) Aluminum Locker Bench.
6	77778:  96” Wide (2,438 mm) Aluminum Locker Bench.
7.	77771-ADA:  42” Wide (1,067 mm) Aluminum ADA Locker Bench.
8.	77771-ADAB:  42” Wide (1,067 mm) Aluminum ADA Locker Bench				 with Back Support.

A.	Unit Heights:
1.	77773, 77774, 77775, 77776, 77777, 77778:
a.	18 inches (457 mm).
2.	77771-ADA
a.	18 inches (457 mm).
3.	77771-ADAB
a.	18 inches (457 mm) seat height.
b.	39 inches (991 mm) back support height.

C.	Unit Depth:
1.	77773, 77774, 77775, 77776, 77777, 77778:
a.	10 inches (254 mm).
2.	77771-ADA:
a.	20 inches (508 mm).
3.	77771-ADAB:
a.	20 inches (508 mm) seat depth.
b.	23 inches (584 mm) back support depth.

D.	Unit Assembly:  Requires minor assembly.

E.	Unit Color: 
1.	Color: Aluminum

2.2	CONSTRUCTION
A.	Locker Bench – Seating area:
1.	Locker shall made of anodized aluminum, 1-3/4 inches (44 mm) in thickness. 
2. 	All corners are to be rounded.

B.	Bench Pedestals:
1.	Pedestals shall consist of aluminum tubing, 3 inches (76 mm) in diameter.
2.	Base shall be ¼” (6 mm) thick aluminum welded to each end of aluminum tubing.
3.	Finished in aluminum powder coat.
C.	Fabricate locker bench parts square, rigid and without warp, with the finished faces flat and free of scratches and chips.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industry's installation instructions.
B.	Anchor the units to the floor through the bench pedestal’s holes:
	1.	Standard bench pedestals:  Four (4) holes.
	2.	ADA-compliant bench pedestals:  Two (2) holes.
C.	Locker benches can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION